
Transportation

As the City of Gardiner  becomes more complex and interwoven with neighboring communitiesand Central Maine grow in population and commerce, the need for a high-quality transportation system becomes increasingly criticalthe region has become more reliant on the local transportation system. . Businesses need transportation to move products and draw in customers; commuters need a way to get to their jobs out of town, and employers need a way to get out of town workers herePeople need safe, reliable forms of transit to support family needs for work, school, shopping, services, and recreation. Businesses, too, depend on a strong transportation system to support employees and the transport of goods and services.. Families need transportation to schools, services, shopping, and recreation.

While the primary mode of transportation in Gardiner and the region is the local roadway system, the City is connected to other communities through interstate highways, a multi-modal trail system and riverfront dock access. Over the past decade, Gardiner has benefited from state and local investments in roads, bridges, sidewalks, and trails to strengthen access in and out of the City.

Roads & Bridges

Road System

Gardiner’s road system has examples of includes roads in each road priority level that the State of Maine utilizes of the Road Priority Classification System – from local road level through interstate highway classifications. The central location and the network of state and local roads make the City highly accessible to many people and businesses throughout the state.. The city is also one of the State Urban Compact Municipalities.	Comment by Guest User: We should define this	Comment by Patricia Hart: This needs a standalone paragraph to explain what it is and why it is important

Table 1: Road Priority Classification System
	Priority
	Definition

	Priority 1 Roads
	[bookmark: _Int_uhUFzkOI]These roads include the Maine Turnpike, the interstate system, and key principal arterials designated as the National Highway System (NHS). The 1,873 miles of Priority 1 highway represent only 8 percent of the road miles in Maine but carry fully 40 percent of all vehicle miles traveled in Mainetraffic.

	Priority 2 Roads
	These roads include high-priority, non-NHS arterials. The HCP 2 roads are high-priority, non-NHS arterials; these second-tier Highway Corridor Priority(HCP 2)
 roads total about 1,252 miles. They represent about 5 percent of the total miles of roadways and carry 18 percent of overall traffic.

	Priority 3 Roads
	These roads generally are the remaining arterials and major collector highways.  These 1,257 miles represent 5 percent of miles and carry 12 percent of the traffic.

	Priority 4 Roads
	These roads generally are the remainder of the major collector highways, minor collector highways, and often also part of the state aid system. These 4,670 miles represent about 20 percent of total miles and carry 17 percent of the traffic.

	Priority 5 Roads
	These roads are local roads and streets and are the year-round responsibility of the municipality. Though they carry just 13 percent of the statewide traffic, these 14,446 miles make up 61 percent of the total miles.


Source: Maine DOT

State Highway’s

Interstate 295 is the only Priority 1 road in Gardiner. It crosses through the southwest corner of the City prior beforeto joining Interstate 95 in West Gardiner.. There are two sets of on and off ramps from I-295 into Gardiner, one from the northbound side and one from the southbound side Interstate 295 is the only Priority 1 road in Gardiner, crossing through the southwest corner of the City. There is a pair of on/off ramps from I-295 into Gardiner where 201 crosses over the highway.. 

U.S. Route 201 is an arterial highway and an important corridor through the Kennebec River region. Rt. 201, also called Brunswick Avenue in Gardiner, connects communities along the Kennebec River from Topsham to the Canadian Border. It is the only U.S. Route in Gardiner. 

[bookmark: _Int_dILfa03T][bookmark: _Int_v4tVa8FM][bookmark: _Int_Y38ifUc7]There are four State Routes in Gardiner, Rt. 9, Rt. 126, Rt. 27 and Rt 24. Routes 9 and 126 overlap are concurrent with each other through Gardiner until they split on the east side of the Kennebec River in Randolph. LThese routes include ocallyLocally named Cobbossee Ave, Water Street and Bridge Street at various points in the City, this is the most heavily traveled corridor in Gardiner. Route 27 forms part of the Pearl Harbor Remembrance Bridge from Gardiner to Randolph. Rt. 27 turns north on the Gardiner side of the bridge, crossing into Farmingdale. These three roads are also classified as State Route 24 that begins in Harpswell and travels north along the Kennebec River crossing into Gardiner from Richmond. Rt. 24 is locally named River Ave and runs through a large portion of the City. Rt. 24 becomes MaineMain Ave at the intersection of Water Street and Church Street. All four State Route’s and U.S. Route 201 all intersect at the Gardiner side of the Pearl Harbor Remembrance Bridge with this also being the terminus of Rt. 24.

Local Roads
The remaining roads in Gardiner, those not classified as Priority 1-3 roads, are a mix of Priority 4 and 5 roads. In the more rural South Gardinerportions ofSouth Gardiner, these roads are key thoroughfares connecting residents to services and each other.	Comment by Guest User: I think it’s more than just South Gardiner; could change to “southern Gardiner” or “rural areas” etc.

One-Way Streets
There are two one-way streets in Gardiner:	Comment by Grainne Shaw: Still true?
· Westerly on Mechanic Street from the intersection of Church Street to the intersection of Brunswick Avenue.
· Easterly on Water Street from the intersection of Bridge Street to the intersection of Church Street.

Regulations for Development and Traffic Growth

Checklist Question: Are conflicts caused by multiple road uses, such as major state or U.S.  route that passes through the community or its downtown and serves as a local service road as well?

Checklist question: Does the community have local access management or traffic permitting measures in place?

Checklist question: Do the local road design standards support the community’s desired land use pattern?

Checklist question: Do the local road design standards support bicycle and pedestrian transportation?	Comment by Guest User: I think we can do better here, and I’ve heard people say they wish the streets were more conducive for these activities. Not sure if they mean Gardiner as a whole or just downtown

[bookmark: _Int_6Y1aTpR1]Checklist question: Do planned or recently built subdivision roads (residential or commercial) simply dead-end or do they allow for expansion to adjacent land and encourage the creation of a network of local streets? Where dead-ends are unavoidable, are mechanisms in place to encourage shorter dead-ends resulting in compact and efficient subdivision designs?

Bridges & Crossings
[bookmark: _Int_rKocQgcF]Gardiner’s road system includes a number ofseveral bridges and water crossings. Many of these are small culverts that are the responsibility of the town to maintain. Culverts must be cleaned and inspected regularly and replaced as necessary. Crossings that have a span of 20 feet or greater are “bridges” in Maine DOT parlance and are the responsibility of the State. Maine DOT inventories all bridges on a regular basis. Each;. E each span receives a Federal Sufficiency Rating – based out of 100 points this numerical score that indicates the health based off four categories:
1. Structural Adequacy and safety
2. Serviceability and Functional Obsolescence
3. Essentiality for Public Use
4. Special Reductions.
Of the twelve bridges in Gardiner, only one, Capen Road, is owned by the city. Five bridges have a federal sufficiency rating under 80, Table 2. A bridge is eligible for federal funding for rehabilitation when it has a rating of less than 80. Should the rating drop below 50, the span is then eligible for federal funding for replacement.  

Table 2: Bridges in Gardiner	Comment by Patricia Hart: Bridge St Maine Ave Winter Street are new bridges - the old ones were removed and replaced in 2020
	Bridge
	Bridge Name
	Owner
	Year Built
	Federal Sufficiency Rating
	Inspection Date

	1533
	RTE. 201/I-295(S.B.)
	MDOT
	1973
	78.7
	6/11/2024

	6318
	RTE 201/I-295(N.B.)
	MDOT
	1973
	90.7
	6/24/2024

	5280
	CAPEN ROAD
	Municipal
	1951
	88.2
	8/1/2022

	1534
	I-295 SB / COBBOSSEE STREAM
	MDOT
	1980
	79.3
	5/22/2023

	6319
	I95 NB/ COBBOSSEE STR.
	MDOT
	1974
	79.3
	4/11/2023

	6023
	ROLLING DAM 2
	MDOT
	1962
	94.2
	8/1/2022

	2605
	NEW MILLS
	MDOT
	2009
	92.3
	8/1/2023

	5070
	WINTER STREET
	MDOT
	1988
	79.8
	8/1/2023

	2101
	BRIDGE STREET
	MDOT
	1918
	81
	5/8/2024

	3098
	MAINE AVE
	MDOT
	1933
	78
	5/8/2024

	0167
	MAINE AVE / MCRR
	MDOT
	1980
	97
	7/17/2024

	2304
	PEARL HARBOR REMEMBRANCE
	MDOT
	1980
	84.7
	6/4/2024


Source: Maine DOT

Traffic Volumes

Traffic Counts
Traffic flows into downtown Gardiner from Farmingdale in the north, Randolph in the east, Route 24 in the southeast, and Brunswick Ave in the south and onto Besides the interstate, only Brunswick Ave/Bridge Street/Maine Ave t intersections. This intersection is the busiest in the city supporting upwards of 14,000 vehicle trips per day with incoming and outgoing traffic. This series of interconnected intersections has been redesigned recently as part of the bridge replacement projects to support more efficient flow of vehicles onto connector roads that lead out of the City. The improvements have reduced the traffic backups on Bridge Street and the Pearl Harbor Bridge. sees more than 10,000 cars per day in Gardiner (Table 3).Besides the interstate, only Brunswick Ave/Bridge Street sees more than 10,000 cars per day in Gardiner (Table 3) Maine DOT collects traffic data including traffic volumes, vehicle classification, and turning movements. The State accomplishes this through two distinct methods: the permanent Continuous Count and short term Coverage Counts at rotating locations. This short term Coverage Count is used to update the Annual Average Daily Traffic (AADT) volume for each road in Maine, which is a standardized metric used for planning, forecasting traffic, analyzing congestion, and allocating funds. In Gardiner, other than the interstate, only Brunswick Ave/Bridge Street sees more than 10,000 cars per day. AADT values for monitored streets from 2019-2023 are shown below(Table 3)
.

Table 3: Annual Average Daily Traffic Counts	Comment by Patricia Hart: Please add in the unit of measure here - vehicle trips per day? etc
	TOWN
	LOCATION
	AADT19
	AADT20
	AADT21
	AADT22
	AADT23

	GARDINER
	I-295 (NB) N/O OFF RAMP TO US 201
	12,790
	-
	-
	-
	-

	GARDINER
	I-295 (NB) S/O OFF RAMP TO US 201
	10,950
	-
	-
	-
	-

	GARDINER
	I-295 (SB) S/O OFF RAMP TO US 201
	10,770
	-
	-
	10,500
	-

	GARDINER
	I-295 (SB) S/O ON RAMP FROM US 201
	13,220
	-
	-
	-
	-

	GARDINER
	I-95 NB OFF RAMP TO US 201
	-
	-
	-
	9,310
	-

	GARDINER
	SR 24 (MAINE AVE) NE/O WATER ST
	-
	-
	-
	-
	7,450

	GARDINER
	SR 24 N/O ARCADE ST @ BR#3098
	-
	-
	-
	-
	7,710

	GARDINER
	SR 24(MAINE AVE) S/O RAMP FROM BRIDGE ST
	-
	-
	-
	-
	8,140

	GARDINER
	SR 27/US 201 (NB) S/O CUT TO BRIDGE ST
	-
	-
	-
	-
	6,080

	GARDINER
	SR 9/126 (COBBOSSEE AV) E/O WEST HILL RD
	-
	-
	-
	-
	8,372

	GARDINER
	SR 9/126 (COBBOSSEE AV) W/O WEST HILL RD
	-
	-
	-
	-
	8,094

	GARDINER
	SR 9/126 (COBBOSSEE) E/O HARRISON AVE
	-
	-
	-
	-
	8,081

	GARDINER
	SR 9/126 (COBBOSSEE) W/O OLD LEWISTON RD
	-
	-
	-
	-
	6,860

	GARDINER
	SR 9/126 (WATER ST) N/O WASHINGTON AVE
	-
	3,840
	-
	-
	6,080

	GARDINER
	SR 9/126 (WATER ST) NE/O CENTRAL ST
	-
	-
	-
	-
	6,420

	GARDINER
	SR 9/126 (WATER ST) NE/O MAPLE ST
	-
	-
	-
	-
	6,245

	GARDINER
	SR 9/126 (WATER ST) SW/O GREEN ST
	-
	-
	-
	-
	6,980

	GARDINER
	SR 9/126 (WATER ST) SW/O MAPLE ST
	-
	-
	-
	-
	6,424

	GARDINER
	SR 9/126 (WATER ST) SW/O SPRUCE ST
	-
	-
	-
	-
	6,140

	GARDINER
	SR 9/126 (WATER ST) SW/O WINTER ST
	-
	-
	-
	-
	6,650

	GARDINER
	SR 9/126(WATER ST) W/O US 201(BRUNSWICK)
	-
	-
	-
	-
	7,010

	GARDINER
	SR 9/126/201 (BRIDGE)(EB) W/O MAINE AVE
	-
	-
	-
	-
	6,234

	GARDINER
	SR 9/126/US 201 (BRIDGE ST) N/O WATER ST
	-
	-
	-
	-
	13,603

	GARDINER
	SR 9/126/US 201 (BRIDGE) SW/O SPRING ST
	-
	-
	-
	-
	14,943

	GARDINER
	SR 9/126/US 201(BRIDGE)(NB) NE/O SPRING
	-
	-
	-
	-
	6,348

	GARDINER
	SR 9/126/US 201(BRIDGE)(SB) NE/O SPRING
	-
	-
	-
	-
	8,563

	GARDINER
	SR 9/27/126 (EB) @ BR#2304 @ RANDOLPH TL
	-
	-
	-
	-
	8,358

	GARDINER
	SR 9/27/126 (WB) @ BR#2304 @ RANDOLPH TL
	-
	-
	-
	-
	8,663

	GARDINER
	US 201 (BRIDGE ST) N/O HIGHLAND AVE
	-
	-
	-
	-
	14,507

	GARDINER
	US 201 (BRUNSWICK AVE) N/O CHURCH ST
	-
	-
	-
	-
	6,580

	GARDINER
	US 201 (BRUNSWICK AVE) NE/O CENTRAL ST
	-
	-
	-
	-
	9,040

	GARDINER
	US 201 (BRUNSWICK AVE) NE/O MARSTON RD
	-
	-
	-
	-
	7,380

	GARDINER
	US 201 (BRUNSWICK AVE) NE/O PIERCE ST
	-
	-
	-
	-
	8,310

	GARDINER
	US 201 (BRUNSWICK AVE) S/O WATER ST
	-
	-
	-
	-
	7,960

	GARDINER
	US 201 (BRUNSWICK AVE) SW/O CENTRAL ST
	-
	-
	-
	-
	8,370

	GARDINER
	US 201 (BRUNSWICK AVE) SW/O MARSTON RD
	-
	-
	-
	-
	7,480

	GARDINER
	US 201 (BRUNSWICK AVE) SW/O MATTSON HTS
	-
	-
	-
	-
	8,200

	GARDINER
	US 201 (BRUNSWICK) S/O LINCOLN AVE
	-
	-
	-
	-
	8,818

	GARDINER
	US 201 NE/O LIBBY HILL RD
	-
	-
	-
	-
	6,830

	GARDINER
	US 201 SW/O LIBBY HILL RD
	-
	-
	-
	-
	6,870

	GARDINER
	US 201 SW/O OLD BRUNSWICK AV (M JCT)
	-
	-
	-
	-
	7,300

	GARDINER
	US 201 SW/O OLD BRUNSWICK RD (S JCT)
	-
	5,140
	-
	-
	6,910


Source: Maine DOT

Safety
A critical element in management of the transportation system is the safe movement of traffic for both vehicles, pedestrians, and alternative modes of transport.

Motor Vehicle Accidents
From 2020 to 2024, there were 618 total vehicle crashes recorded. in Gardiner. Accidents were more common in the fall and winter months and at times corresponding to the end of the typical workday, between 4:00 pm and 5:00 pm.	Comment by Guest User: How does this compare to other similarly-sized towns and the State as a whole?

Figure 1: Crashes by Month from 2020-2025

Source: Maine DOT


High Crash Locations
Records are kept of vehicle accidents and areas along the highway system which are marked as High Crash Locations (HCL). MDOT defines an HCL as a roadway intersection or segment which experiences eight or more accidents in a 3-year period and has a Critical Rate Factor (CRF) more than 1.00. CRF is a measure of the actual number of accidents compared to the theoretical accident experience that would normally be expected in that situation.	Comment by Patricia Hart: Who keeps the records?

From 2022 to 2024 there were three HCL in Gardiner 

Table 4: High Crash locations in Gardiner 2022-2024
	Location
	Total Reported Crashes
	Percent Injury

	 Int of COBBOSSEE AV  W HILL RD
	9
	11.1

	 Int of BRIDGE ST  HIGHLAND AV
	8
	0

	 Int of BRIDGE ST  MAINE AV  STATE HWY 27
	33
	30.3


Source: Maine DOT

Parking
On-street Parking
The City allows on-street parking during the day and overnight in many neighborhoods from April until November. During winter months, cars may be towed if parked after dark. As the state legislature enacts laws that removed local requirements for off-street parking for dwelling units, there will be more issues with cars left on the streets overnight in the winter months.

Municipal Parking Lots
There is one are five municipally owned/operated parking lotslot in Gardiner,, the accessible by Arcade Parking Lot, the Waterfront Parking Lot, the City Hall Parking Lot, the Bailey Lot, and the Park and Ride on Route 201 and Interstate I-95. In addition to these lots there are several privately owned parking lots for customers of the lot owner. Those include Hannaford Parking Lot, the Depot Parking Lot, Tiger Town Parking Lot, Camden National Parking Lots, Reny’s Parking Lot, and the Library Parking Lot. Street.Street. Patrons of the shops and restaurants utilize it when on street parking is at capacity, as do the residents of the homes on Water Street.These lots as well as private dedicated parking spaces support the downtown residents, businesses, and patrons. 

Checklist Question: List and locate municipal parking areas including capacity, and usage.	Comment by Guest User: How many parking spots are available at the Arcade St. lot?
KVCOG did an inventory of parking spaces in 2019. The Reny’s Lot, Bailey Lot, and Camden Lots have been added since that time.

Checklist Question: Are there parking issues in the community? If so what are they?

With the opening of the restored Johnson Hall Opera House 400 seat theater, people were concerned about the sufficiency of parking. During the first two years of operation there have been minimal problems with parking.Johnson Hall, Gardiner Main Street, and the City created parking maps for patrons that are emailed to ticket holders prior to each show.

At various times, concurrent events have brought thousands of people to the city. The existing parking, including in nearby Church parking lots, has been adequate. Hannaford has been neighborly in allowing public parking in the far reaches of their lot. Boaters use these spaces in the summer to park their trucks with boat trailers.

Checklist Question: If there are parking standards, do they discourage development in village or downtown areas?
Section 11 of Gardiner’s Land Use Ordinance covers Roads, Traffic Access and Parking Standards. The standards do not require on-site or designated parking in the traditional downtown area. Recent changes to state law have eliminated most parking requirements for dwelling units.
Public Transportation
Gardiner is not currently served by any public transportation systems. While previously served by the Kennebec Explorer, a program from of the Kennebec Valley Community Action Program, that service ceased operation January 1, 2024. Transportation KVCAP will provide transportation for medical services is available for eligible clients. who have completed an application.

Bicycle & Pedestrian Facilities	Comment by Patricia Hart: Need to add a paragraph on the Merry Meeting Trail
Rail Trail
The Kennebec River Rail Trail is a 6.5-mile public path that runs along the Kennebec River from Gardiner to Augusta. The trail is open year-round for walking, running, biking, and more. Many use this trail to commute from Gardiner to adjacent towns for work and/or pleasure. This will be discussed more in depth in the Recreation Chapter.

Sidewalks	Comment by Grainne Shaw: I know a lot of conversation has been had about the sidewalks in town but I have no details. What about the sidewalks through the neighborhoods? South Gardiner?
Much of the high-density neighborhoods in Gardiner is accessible throughby sidewalks. Pedestrians can access all of Downtown Gardiner by foot as well as a large swath of the most of the densely populated residential areas. South Gardiner also has sidewalk facilities in its high density residential neighborhoods. stretching from XXX to XXX. 

One known issue with pedestrian use is the state of the sidewalks through Gardiner’s Downtown. Over time, the brick sidewalks which are comprised of bricks have shifted and broken, causing significant challenges for those using mobility aids, strollers, and other wheeled devices.

In 2007, the Gardiner Sidewalk Committee inventoried all of the sidewalks in Gardiner on a scale of 1-5 (1: Low Attention, 5: High Attention), and created a recommended work list for all sidewalks that scored 3.5 or higher. The committee recommended a $628,000 bond to pay for these improvements, which was finally adopted and bonded by Council in 2014.,, while proposed, failed to pass the Gardiner City Council. Of the 61 recommended sidewalk improvements, two several have been completed:
· Rte. 126 – West Street to Middle School 
· New Mills Bridge to West Street Rte. 126.
· Washington Ave
· Brunswick Ave – one side from Bridge to Laura Richards School
· Vine Street to Water Street
· Highland Avenue
· Spring Street
· Church Street
· Arcade Street to Water Street– extension of the KRRT
· New pedestrian bridge – part of the bridge replacement project

Wright-Pierce worked with the City of Gardiner in 2008 to create a “bundled projects” plan, which included sidewalk improvements. The project areas focused on the downtown area, along the CobbosseeCobbossee Stream. Recommended sidewalk improvements included:
· Removal and Replacement of Sidewalk Surfaces
· Replace and Add Curbing
· Restore Esplanades
· Crosswalk Connections
· Repair Brick Sidewalks
· Traffic Control
· Unit Price Contract

Checklist Question: To what extent do sidewalks connect residential areas with schools, neighborhood shopping areas, and other daily destinations?


The largest generator of regular pedestrian traffic in Gardiner is the schools. All schools in the city are accessible by sidewalks, as such they see the highest level of use before and after regular hours from September through June. Events such as holiday parades, festival’s, and street markets contribute to large numbers of pedestrian traffic throughout the year. 	Comment by Patricia Hart: Are pedestrians from the neighborhoods. Students rarely walk.

People living in the high-density neighborhoods as well as downtown residents are the most active users of the sidewalks. They use the sidewalks to walk to the grocery store, shops, services, and restaurants. Many people, particularly older people, walk the neighborhoods as well as use the park walkways for exercise. While once used by students, very few students use sidewalks to walk to school.

Checklist Question: Identify major traffic (including pedestrian) generators, such as schools, large businesses, public gathering areas/activities, etc. and related hours of their operations.

The Bridge Street area can be the most congested roadway and pedestrian way in the morning and evening hours. Several connectors join to cross over the bridge into Gardiner and other connectors flow from the north and south onto the street. This is a weekday daily occurrence.

For gatherings and public events, the downtown with Johnson Hall, dance studios, a gaming store, and restaurants can generate sporadic traffic use that requires hours long parking. Pedestrians perambulate in and around the downtown and waterfront park regularly.
Rail Lines
There are no active rail lines in Gardiner. While there are tracks running following that follow the line of the Kennebec River, the line has been removed in some locations and paved over in others rendering it near obsolete.

Airport
Gardiner is served by Augusta State Airport, eight miles to the north, and Portland International Jetport, 55 miles to the south, and Bangor Airport to the north 90 miles. 

Transportation Planning
Checklist Question: What are the transportation system concerns in the community and region? What, if any, plans exist to address these concerns?

Beginning in October 2025, the City of Augusta is conducting a city-wide transit study focusing on alternatives modes of transit. Gardiner should be involved where feasible to encourage regional progress towards connectivity options and solutions..	Comment by Guest User: This feels more like a policy than an inventory component. Do we know how we can plug into this study? That may be more appropriate here.  

Checklist Question: How do state and regional transportation plans relate to your community?

Regional and Statewide Trends
There are increasing trends regionally and statewide to utilize use alternative modes of transportation such as bicycles, and motorized bicycles and scooters. Gardiner is well situated to take advantage of these changes with easy access to the Kennebec River Rail Trail and extensive sidewalk system. However, there are inherent conflicts in adding motorized vehicles to pedestrian passageways that must be managed.. 	Comment by Patricia Hart: No bikes, e-bikes or scooters are allowed on pedestrian sidewalks - too dangerous

Financial Resources

More than any other public service, the transportation system is heavily connected with events and plans outside of municipal boundaries impacted by state and federal investment decisions. Recent cut backs in state and federal funding have made it difficult for the City to invest properly in its transportation system. Decades of deferred maintenance have left many roads, culvert systems, and sidewalks in disrepair.. Economic At the same time regional population growth and the increasing reliance on vehicle transportation is likely to increase the strainingstrain on the existing transportation roadway system in Gardiner due to growing populations both in the City and surrounding communities.

Financial Resources
The transportation system is costly to maintain. The system is in a constant state of deterioration, and deferring maintenance accelerates the pace and costs of repair. Even without improvements, the roads in XXXXX require close to $$$$$$ dollars a year in upkeep.

Checklist question: What is the community’s current and approximate future budget for road maintenance and improvement?
John Cameron


Transportation Talking Points
1. The loss of the Kennebec Explorer is significant. With no public transit system in place to replace that asset, resource residents of Gardiner are reliant on taxi services or their own personal vehicles.

2. The opportunity for people to walk within the older, built-up portion of the City exists but the overall “walkability” within this area needs to be improvedThe City should continue to address the aging sidewalks to make them safer for the many people who use them..

Checklist Question: Do available transit services meet the current and foreseeable needs of community residents? If transit services are not adequate, how will the community address the needs?

Crashes by Month 2020-2024

Month	 JANUARY  	 FEBRUARY 	 MARCH    	 APRIL    	 MAY      	 JUNE     	 JULY     	 AUGUST   	 SEPTEMBER	 OCTOBER  	 NOVEMBER 	 DECEMBER 	61	55	39	37	45	50	37	41	54	65	64	70	Month
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